Module:
SEQUENZA 10 N FR     Version:3.2

For use with Linear Phase Sequenza Setups

For fullrange applications without additional subwoofer(s)

Module Outputs:
   LF:        Use this output for LF driver
                The LF driver is connected at 1+1-
			   
   LF/HF:    Use this output for LF/HF speaker
                 The LF/HF speaker is connected at 2+2-
			      

Switchable filters included:
   SEQ10 Straight - For straight array (0 - 2 deg.)

   4-5x SEQ10 - Array Filter depending to array length
                       (further filters are available - EQ Overlay Store/Recall)
   
   SEQ10 HBoost 1.5dB - HF boost for far field applications
                                      (further filters are available - EQ Overlay Store/Recall)
   