Module:
PIA LFX BR Overlap     Version:1.0

For fullrange applications using PIA M and PIA LFX
Crossover frequency is set to 200 Hz

Module for Cardioid Setup of the PIA M (check back of speaker for instructions)

Switchable filters included:
   PIA LFX - 60Hz CUT: For high SPL applications and additional subwoofer(s) in 60 Hz mode