Module:
PIA M BR FR     Version:1.0

For fullrange applications without additional subwoofer(s)

Module for Bass Reflex Setup of the PIA M (check back of speaker for instructions)

Adjust HF Spread on back of speaker according to venue needs and apply switchable filter accordingly.

Switchable filters included:
   PIA M HF medium - for medium spread of adaptive high frequency array

   PIA M HF wide - for wide spread of adaptive high frequency array