Module:
SPECTRA 212 XW LS LCut     Version:1.9

LowCut Module for applications with additional subwoofer(s)

Module Outputs:
   LF/HF:    Use this output for LF/HF driver
                The LF/HF driver is connected at 1+1-
			   
   MF:       Use this output for MF speaker
                The MF speaker is connected at 2+2-
			      

Switchable filters included:

	SingleLineSource - Adaptation Filter for a Single Spectra 212 in Line Source Mode
	                             BE ADVISED: Set the rearward switch to "Point Source Mode"

	2x S212 LCut - Array Filter for Clusters of 2x K&F SPECTRA 212 LCut

	3x S212 LCut - Array Filter for Clusters of 3x K&F SPECTRA 212 LCut

	4x S212 LCut - Array Filter for Clusters of 4x K&F SPECTRA 212 LCut